* **WC-1 WATER CLOSET WHEELCHAIR**
  + - AMERICAN STANDARD 3461.001.020 MADERA ELONGATERD UNIVERSAL FLOOR MOUNTED ADA 17IN RIM WHITE BOWL
    - AMERICAN STANDARD 606B121.002 1.28 GPF FLUSH VALVE SELECTRONIC EXPOSED AC BASE MODEL
    - AMERICAN STANDARD PK00.HAC HARD-WIRE TRANSFORMER WITH 10IN EXTENSION CABLE
    - AMERICAN STANDARD 5901110T.020 HEAVY DUTY ELONGATED OPEN FRONT SEAT LESS COVER WITH EVERCLEAN SURFACE
* **WC-2 WATER CLOSET WHEELCHAIR**
  + - AMERICAN STANDARD 3462.001.020 MADERA ELONGATED UNIVERSAL BOWL WITH BED PAN LUGS
    - AMERICAN STANDARD 6047.820.002 BEDPAN WASHER ASSEMBLY WITH STRAIGHT DOWN TUBE 1.28 GPF
    - AMERICAN STANDARD 5901110T.020 HEAVY DUTY ELONGATED OPEN FRONT SEAT LESS COVER WITH EVERCLEAN SURFACE
* **WC-3 WATER CLOSET BARIATRIC**
  + - AMERICAN STANDARD 3461.001.020 MADERA ELONGATERD UNIVERSAL FLOOR MOUNTED ADA 17IN RIM WHITE BOWL
    - AMERICAN STANDARD 6047.820.002 BEDPAN WASHER ASSEMBLY WITH STRAIGHT DOWN TUBE 1.28 GPF
    - AMERICAN STANDARD 5901110T.020 HEAVY DUTY ELONGATED OPEN FRONT SEAT LESS COVER WITH EVERCLEAN SURFACE
* **L-1 LAVATORY**
  + - AMERICAN STANDARD 7500.180.002 4IN CC 4IN WB HANDLES 1.5 GPM GOOSENECT LAVATORY FAUCET
    - MCGUIRE 155A8 PO PLUG 1-1/4X8IN TAIL PIECE
    - DEARBORN 507-1 1-1/4 SEMI-CAST P-TRAP WITH CLEANOUT CHROME
    - KEENEY 2622PCLKLF ANGLE STOPS 5/8X3/8 1/4 TURN LOOSE KEY LEAD FREE
    - EZ-FLO 48004 STAINLESS STEEL 1/2FX3/8COMP 16IN LONG X 5/16IN ID SUPPLIES
    - EZ-FLO 25711 ESCUTCHEONS 1/2 CTS 5/8 OD ESC LOW PAT 2-1/2 OD
    - IPS 82193 102EZ ADA PTRAP COVER KIT WITH 2 VALVES
    - HONEYWELL UMV500-LF/U 3/8 TMV UNIVERSAL UNDERSINK THERMOSTATIC MIXING VALVE LEAD FREE 3 OR 4 PORT
* **L-2 LAVATORY**
  + - AMERICAN STANDARD 0355.012.020 WHITE WALL HUNG LUCERNE LAVATORY WITH 4IN CENTERSET
    - AMERICAN STANDARD 7500.180.002 4IN CC 4IN WB HANDLES 1.5 GPM GOOSENECT LAVATORY FAUCET
    - MCGUIRE 155A8 PO PLUG 1-1/4X8IN TAIL PIECE
    - DEARBORN 507-1 1-1/4 SEMI-CAST P-TRAP WITH CLEANOUT CHROME
    - KEENEY 2622PCLKLF ANGLE STOPS 5/8X3/8 1/4 TURN LOOSE KEY LEAD FREE
    - EZ-FLO 48004 STAINLESS STEEL 1/2FX3/8COMP 16IN LONG X 5/16IN ID SUPPLIES
    - EZ-FLO 25711 ESCUTCHEONS 1/2 CTS 5/8 OD ESC LOW PAT 2-1/2 OD
    - HONEYWELL UMV500-LF/U 3/8 TMV UNIVERSAL UNDERSINK THERMOSTATIC MIXING VALVE LEAD FREE 3 OR 4 PORT
    - IPS 82193 102EZ ADA PTRAP COVER KIT WITH 2 VALVES
      * WATTS TCA-411 FLOOR MOUNTED LAVATORY CARRIER WITH CONCEALED ARMS
* **S-1 SINGLE COMPARTMENT SINK**
  + - JUST SL-1921-A-GR-3 18GA 1 COMPARTMENT SINK
    - AMERICAN STANDARD 6403170.002 MONTERREY 1.5 GPM 8IN CC GOOSENECK WRIST BLADE HANDLE FAUCET LESS SPRAY
    - DEARBORN 815B FLAT TOP SINK BASKET STRAINER
    - DEARBORN 510-1 1-1/2 SEMI-CAST P-TRAP WITH CLEANOUT CHROME
    - KEENEY 2622PCLKLF ANGLE STOPS 5/8X3/8 1/4 TURN LOOSE KEY LEAD FREE
    - EZ-FLO 48005 STAINLESS STEEL 1/2FX3/8COMP 20IN LONG X 5/16IN ID SUPPLIES
    - EZ-FLO 25711 ESCUTCHEONS 1/2 CTS 5/8 OD ESC LOW PAT 2-1/2 OD
* **S-2 SINK**
  + - JUST SL-17519-A-GR-4 1 COMPARTMENT STAINLESS STEEL KIT SINK
    - AMERICAN STANDARD 6408.140.002 1.5 GPM FAUCET
    - DEARBORN 815B FLAT TOP SINK BASKET STRAINER
    - DEARBORN 510-1 1-1/2 SEMI-CAST P-TRAP WITH CLEANOUT CHROME
    - KEENEY 2622PCLKLF ANGLE STOPS 5/8X3/8 1/4 TURN LOOSE KEY LEAD FREE
    - EZ-FLO 48005N STAINLESS STEEL 1/2FX3/8COMP 20IN LONG X 5/16IN ID SUPPLIES
    - EZ-FLO 25711 ESCUTCHEONS 1/2 CTS 5/8 OD ESC LOW PAT 2-1/2 OD
* **S-3 SOILED UTILITY SINK**
  + - JUST SLX-17519-A-GR-3 17-1/2X19 18GA 10IN DEEP STAINLESS STEEL SINK
    - AMERICAN STANDARD 6540.180.002 8IN 2 HANDLE WIDESPREAD LAVATORY FAUCET 1.5GPM
    - DEARBORN 510-1 1-1/2 SEMI-CAST P-TRAP WITH CLEANOUT CHROME
    - KEENEY 2622PCLKLF ANGLE STOPS 5/8X3/8 1/4 TURN LOOSE KEY LEAD FREE
    - EZ-FLO 48004 STAINLESS STEEL 1/2FX3/8COMP 16IN LONG X 5/16IN ID SUPPLIES
    - EZ-FLO 25711 ESCUTCHEONS 1/2 CTS 5/8 OD ESC LOW PAT 2-1/2 OD
* **MS-1 MOP SINK**
  + - FIAT TSB-3010 TERRAZZO MOP SERVICE SINK 24X24X12 WITH STAINLESS STEEL THRESHOLD
    - AMERICAN STANDARD 8354.112.002 EXPOSED YOKE WALL-MOUNT UTILITY FAUCET
      * JONES STEPHENS M05-001 SERVICE SINK HOSES WITH STAINLESS BRACKET
    - JONES STEPHENS M05-003 STAINLESS STEEL 3 BRACKET MOP HOLDER
    - FIAT MSG2424 MOP SINK WALL GUARD STAINLESS STEEL 24X24
* **SH-1 SHOWER**
  + - COMFORT DESIGNS SSB3838TR.75CTBD-PAN 38IN X 38IN SOLID SURFACE SHOWER PAN
    - COMFORT DESIGNS 1DRA101 2IN BRASS NO CAULK SHOWER WITH STAINLESS STEEL STRAINER
    - POWERS E710-0-0-0-8-0-W HAND SHOWER SYSTEM
* **SH-2 SHOWER**
  + - COMFORT DESIGNS SSB6238TR.75CTB-PAN 62IN X 38IN SOLID SURFACE SHOWER PAN
    - COMFORT DESIGNS 1DRA101 2IN BRASS NO CAULK SHOWER WITH STAINLESS STEEL STRAINER
    - POWERS E710-0-0-0-8-0-W HAND SHOWER SYSTEM
* **CSS-1 CLINIC SERVICE SINK** 
  + - AMERICAN STANDARD 9512.999.020 25-1/4X21-1/8 WALL HUNG CLINIC SERVICE SINK
    - AMERICAN STANDARD 7832.512.075 STAINLESS STEEL RIM GUARD COMES WITH A QUANTITY OF 2
    - AMERICAN STANDARD 8345.115.002 EXPOSED YOKE WALL MOUNTED UTILITY FAUCET WITH TOP BRACE & ROUGH CHROME FINISH
    - AMERICAN STANDARD 7880.124.002 BED PAN CLEANER ASSEMBLY
    - AMERICAN STANDARD 6047.117.002 FLUSH VALVE EXPOSED MANUAL CLINIC SINK 6.5GPF
      * WATTS ISCA-550 SERIES HORIZONTAL ADJUSTABLE CLOSET CARRIER